REQUIREMENTS DOCUMENT

**Project:** ECSE 211 Final Design Project – Team 6

**Document Version Number**: 6.0

**Creation Date:** 14/10/2017

**Original Author:** Alex Hale

**Edit History:**

[14/10/2017] Frederic Cyr: set up the format of the document.

[16/10/2017] Alex Hale: added content from project specifications; changed version system to

WEEK.EDIT (e.g. it is currently week1, edit 2 => 1.2).

[22/10/2017] Alex Hale: transferred to Word document for easier formatting; minor revisions

[30/10/2017] Alex Hale: resolved Scope TODOs

[4/11/2017] Alex Hale: changed to present tense; various minor changes

[19/11/2017] Alex Hale: minor updates after being informed of final competition details

1. TABLE OF CONTENTS
2. Capabilities
   1. Purpose
   2. Scope
   3. Constraints
   4. User Functions
   5. Operating Environment
   6. Performance
3. Compatibility
   1. Component Reuse
   2. Compatibility with Third Party Products
4. Glossary of Terms
5. CAPABILITIES
   1. PURPOSE

Create an autonomous vehicle capable of navigating around an obstacle course, crossing a zip line, finding and recognizing coloured blocks, and returning to the starting corner.

* 1. SCOPE

*Size of Area*:

* + 12x12 grid of squares, each with a side length of 30.48cm

*Capabilities of Robot*:

* + receive parameters from the game control server
  + localize in starting square
  + navigate around the playing field
  + traverse a zipline
  + find a block of a specified colour in the given zone
  + beep three times
  + return to the starting corner along a specified path

*Time Limits*:

* + 30 seconds to localize
  + 5 minutes to complete the run

*Tolerance on Robot Capabilities*:

* + navigate with enough accuracy to mount the zip line
    - the robot will only mount the zip line if the zip line wheel is aligned with the zip line within a 4o margin of error in either direction
  + differentiate between colours of blocks
  1. CONSTRAINTS

See Constraints Document.

* 1. USER FUNCTIONS

The user may interact with the device before it operates, but once the robot is given to the TA to be placed on the field, the robot must act entirely autonomously. The user can operate the device using the keypad on the front of the brick.

* 1. OPERATING ENVIRONMENT

The robot operates on the playing field, which is a 12x12 grid of squares, each with side length 30.48cm. The surface of the field is beige wood, with black grid lines separating each square to help the robot navigate. The lighting of the environment is variable, so the performance of the colour sensors is carefully calibrated. The competition is held indoors, so any other external environmental factors are negligible.

* 1. PERFORMANCE

Since user input only occurs before the start of the trial, response time to commands need only be fast enough to make testing easy for the user. Other time limits and travel requirements are outlined in Section 2.2 - Scope. The travel speed of the robot has no explicit requirements, but faster is better - the faster one can go without making errors, the higher the probability of completing the game before the opposing robot.

1. COMPATIBILITY
   1. COMPONENT REUSE

Any hardware or software created during the Research and Development phase (Labs 1 through 5) can be reused. However, it is important to ensure that those components do not pose restrictions on the robot. For example, all the hardware designs in the labs required fewer sensors than are required on the final robot. The most important existing components that are reused are the LEGO Mindstorms EV3 set and the leJOS library.

* 1. COMPATIBILITY WITH THIRD PARTY PRODUCTS

The robot hardware is entirely made up of LEGO parts, so the frame does not have to interface with components from other suppliers. The robot's sensors are calibrated for the wooden floor and coloured blocks that are part of the competition, both of which are made available before the competition. The robot’s zip line arm must be at the correct height to interface with the zip line. Some custom structural pieces can be 3D printed specifically for the robot if needed.

1. GLOSSARY OF TERMS

None required.